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Application Form for Security/Insurance Bond Release.



	Developer's Name
	

	Developer's Address: Telephone No:
	

	Location of Development
	

	Development Name
	

	Planning Reference Numbers:
	

	Management Company Name:
	

	Management Company Contact Details:
	

	Roads	(metres)
	Length:	m.
	Width:	m.

	Footpaths: (metres)
	Length:	m.
	Width:	m.

	Foul Sewers:
	Lengths (m)
	Diameter (mm)
	Material

	
	
	
	

	
	
	
	

	
	
	
	

	
	
	
	

	Number of Foul Sewer Manholes:
	No.

	Surface Water Sewers:
	Lengths (m)
	Diameter (mm)
	Material

	
	
	
	

	
	
	
	

	
	
	
	

	
	
	
	

	Number of Surface Water Sewer Manholes & Road Gullies
	Manholes 	No.
	Road Gullies 	No.

	Sewer Connection Permit Receipt No. & Permit No.
	

	Watermains
	Length (m)
	Diameter (mm)
	Material
	Class

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	Water Connection Fee receipt No:
	



1

	Area of Open Space:
	

	Area of Development:
	

	No. of Houses:
	

	Housing Density per Hectare:
	

	Size of Water Meter:
	

	Details of surface-water or sewage pump(s)
	

	No. of Public Lights:
	

	Development Levy Receipt No.
	

	Security Bond:
	Amount €
	Expiry Date:

	Development Commencement Date:
	
	




As-Constructed Drawings and CCTV survey of sewers to be enclosed with this Form.

As Constructed Drawings (“As-builts”) completed by:



Qualifications:  	
Drawings to be certified by a bonded chartered civil engineer / consulting engineer or bonded / certified architect.


Drawings and CCTV Format.

The “as constructed” drawings shall consist of 3 sets of four separate drawings of scale 1:500 that will detail the following information:


Drawing 1:

The portion of the development bounded by a red line, and shall indicate roads, footpaths, public lighting and road gullies. The location of all other services which may include Electrical ducting/ poles, Gas, Cablelink/ NTL, Broadband and telecom ducting/ poles shall be included on the “as constructed drawings”

Drawing 2:
The portion of the development bounded by a red line, and shall indicate watermains layout.
Watermains layout to show watermeter location, watermain diameter, watermain class and include location of bulk meters, Water Meter Boundary Box/ manifold units/ stopcocks, valves and hydrants.

Drawing 3:

Sanitary services layout to show layout and longitudinal sections of foul sewers, surface water sewers, diameters/ materials, location of connection to public sewers, location of surface-water discharge points, manholes and road gullies. The invert level and cover level of all manholes shall be clearly shown in plan and section and relate to the Malin Head datum.

Drawing 4: Map depicting the open space coloured green, and shall detail any services that traverse the open space.

Applicant to submit three copies of each drawing, and submit drawings on CD (Autocad format).



CCTV Survey of Sewers.

A CCTV survey/manhole survey of the sewer systems prepared to SUS 25 electronic format shall be submitted to Galway City Council with this Form.

The survey shall be completed at the developer's / owner's / applicant's expense.

The sewers to be surveyed shall be thoroughly cleaned out prior to survey.

The CCTV Survey shall be carried out using a camera which is capable of measuring and recording distances between manholes.

The CCTV survey report shall conform to the standards set out in the WRC Manual on Sewer Condition Classification. All defects identified in the developer's initial inspection of the sewerage systems shall be repaired and made good by the developer prior to submission of CCTV survey to GCC. In the event of any defects remaining, such defects shall be repaired by the Developer at his/her own expense as a prerequisite to GCC approving the release of the Security Bond. The hard-copy report shall be supplemented by high-resolution photographs and quality recordings submitted on CD-Rom or DVD or memory stick.

The invert and cover levels of the manholes shall be indicated relative to Malin Head Ordnance Datum.



Developer to provide Galway City Council with the following where applicable:

· Evidence that any necessary Wayleaves / Consent to Access for Galway City Council's unfettered access to Services are reserved in perpetuity in the transfer documentation to house purchasers,

· Copy of receipts and GCC confirmation that all levies and development contributions have been paid in full.

· Copy of the agreed Bond for the development,

· Copy of any correspondence from GCC or other agency with regard to site instructions or field change orders which occurred during the construction phase.


Galway City Council inspection of Works, Snag-list etc.

Where the development/estate/ apartment block is found on initial inspection by GCC to be incomplete and/or not up to the required standard, then any subsequent inspection by GCC will carry a charge of €300 per inspection, until such time as the Release of Bond is recommended.


A note on the Multi-Unit Developments Act 2011.

The Multi-Unit Developments Act 2011 came into force on 01 April 2011. This Act is applicable to both new and existing multi-unit developments. A multi-unit development is defined as a development comprising at least 5 residential units. It may also have a commercial element in which case it is referred to as a mixed multi- unit development.

Under section 7 of the Act, obligations to complete the development remain with the developer: The transfer of the ownership of an interest in the relevant parts of the common areas of a multi-unit development shall not relieve the person who would otherwise have been responsible from the duty, obligation or responsibility to ensure completion of the development, including -

(a) compliance with the requirements or conditions of a planning permission under the Planning and Development Acts 2000 to 2009 which relates to the development concerned, and

(b) compliance with the Building Control Acts 1990 and 2007.


Certification.

Certification below applies to As-constructed Works only.

Form DS 1 (2013)
CERTIFICATION.

AS-BUILT Works:

Certificate No. 1

Certification to be by a bonded Chartered Civil Engineer / Consulting Civil Engineer. A copy of his/her/company PROFESSIONAL INDEMNITY INSURANCE shall be attached to this Form.


To: Galway City Council,


This is to certify that:

· All sewers are connected to separate systems, i.e. foul to foul and surface water to surface water,
· All sewers and drainage pipes for connection to the public sewer /drainage system have been designed and constructed in accordance with the requirements of Section 3 , "Sewers and Drains" of "Recommendation for Site Development Works for Housing Areas” published by the Department of the Environment, and Part H of the Building Regulations, applicable at time of construction.

· All Roads and footpaths have been designed and constructed in accordance with the requirements of Section 2, “Roads and Footways” of “Recommendation for Site Development Works for Housing Areas” unless specified and required otherwise by Galway City Council.

· The Water Supply system has been designed and constructed in accordance with the requirements of
· “Recommendation for Site Development Works for Housing Areas", Section 4, “Water Supply”
· Part G of the Building Regulations,
· BS EN 806 – 2: 2005 “Specification for installations inside buildings conveying water for human consumption”.
· 	An independent technical audit of the water distribution system has been prepared by a specialist water network management company; Report attached.

· 	The public lighting scheme as installed is fully compliant with relevant standards, regulations and statutory instruments; certification(s) attached.



Signature: 		Date: 	


Name:	 	

Professional Qualifications:  	
Professional Indemnity Insurance reference: 	




(attach copy).

Form DS 1 (2013)

CERTIFICATION.

AS-BUILT Works:

Certificate No. 2

Certification to be by a bonded Chartered Civil Engineer / Consulting Engineer / Architect / Planner. A copy of his/her/company PROFESSIONAL INDEMNITY INSURANCE shall be attached to this Form.



To: Galway City Council,


This is to certify that:

The Development 	has been constructed to the appropriate specified standards, and in full compliance with the Planning Permission granted; Planning Register Reference 		.




Signature: 		Date: 	


Name:	 	

Professional Qualifications:  	
Professional Indemnity Insurance reference: 	




(attach copy).

Form DS 1 (2013)


CERTIFICATION.

AS-BUILT Works:

Certificate No. 3

Certification to be by a bonded registered landscape architect (Irish Landscape Institute) or bonded chartered landscape architect (UK Landscape Institute). A copy of his/her/company PROFESSIONAL INDEMNITY INSURANCE shall be attached to this Form.



To: Galway City Council,


This is to certify that:

Open spaces and landscaping have been completed in full compliance with the Planning Permission(s) granted, with the written approval of the Parks Section of the Transportation, Infrastructure, Recreation and Amenity Department of Galway City Council.







Signature: 		Date: 	


Name:	 	

Professional Qualifications:  	
Professional Indemnity Insurance reference: 	




(attach copy).


Completed forms and stated requirements shall be submitted to:

Galway City Council,
Planning Office, 
City Hall, 
College Road 
Galway.
H91 X4 K8
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